Jump to main content

##

# 2.5.4 AFECx_ChannelsInterruptEnable Function

## C

    void AFECx_ChannelsInterruptEnable (AFEC_INTERRUPT_MASK channelsInterruptMask) // x - Instance of the AFEC peripheral

## Summary

Enables the ADC interrupt sources

## Description

This function enables interrupt sources specified in channelsInterruptMask.

## Precondition

AFECx_Initialize() must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
channelsInterruptMask | interrupt sources

## Returns

None.

## Example

    AFEC0_Initialize();
    AFEC0_ChannelsInterruptEnable(AFEC_INTERRUPT_EOC_0_MASK);

## Remarks

This function does not disable interrupts which are not included in the mask.