Jump to main content

##

# 2.79.6 PCR_PrivilegeDisablex Function

## C

    /* x = Privilege Enable Register number */

    void PCR_PrivilegeDisablex (PCR_PRIV_ENx blockId)

## Summary

Enables access to the given peripheral block in all modes

## Description

Enables access to the given peripheral block in all modes

## Precondition

None

## Parameters

Param | Description
--- | ---
blockId | One of the peripheral block ID from the PCR_PRIV_ENx Enum

## Returns

None

## Example

    PCR_PrivilegeDisable0(PCR_PRIV_EN0_GPIO);

## Remarks

None