Jump to main content

##

# 2.75.12 OPA_OFFSET_INPUT_TYPE Enum

## C

    typedef enum
    {
        OPA_PMOS_OFFSET_IN_HIGH_POWER_MODE,     /**< Offset Correction for PMOS Differential Input Pair (High-Power mode) */
        OPA_NMOS_OFFSET_IN_HIGH_POWER_MODE,     /**< Offset Correction for NMOS Differential Input Pair (High-Power mode) */
        OPA_PMOS_OFFSET_IN_LOW_POWER_MODE,      /**< Offset Correction for PMOS Differential Input Pair (Low-Power mode) */
        OPA_NMOS_OFFSET_IN_LOW_POWER_MODE       /**< Offset Correction for NMOS Differential Input Pair (Low-Power mode) */

    } OPA_OFFSET_INPUT_TYPE;

## Summary

Enumeration for selecting the offset correction type for the OPA module.

## Description

This enumeration defines the possible offset correction types for the OPA module, allowing the selection of different input pairs and power modes for offset correction.

## Remarks

None.