Jump to main content

##

# 2.4.16 ADCHS_EOSCallbackRegister Function

## C

    void ADCHS_EOSCallbackRegister (uintptr_t context)

## Summary

Registers the function to be called from end of scan interrupt

## Description

This function registers the callback function to be called from end of scan interrupt

## Precondition

ADCHS_Initialize() must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
context | Allows the caller to provide a context value (usually a pointer to the callers context for multi-instance clients)

## Returns

None.

## Example

    void ADCHS_Callback_Fn(uintptr_t context)
    {
    }

    ADCHS_Initialize();
    ADCHS_EOSCallbackRegister(ADCHS_Callback_Fn, NULL);

## Remarks

Context value can be set to NULL if not required. To disable callback function, pass NULL for the callback parameter.