Jump to main content

##

# 2.124.5 TMR1_PeriodGet Function

## C

    uint16_t TMR1_PeriodGet(void);

## Summary

Reads the period value of given timer.

## Description

This function reads the value of period of given timer.

## Precondition

TMR1_Initialize() function must have been called first.

## Parameters

None.

## Returns

period - The timer's period value.

## Example

    uint16_t period;

    TMR1_Initialize();
    period = TMR1_PeriodGet();

## Remarks

None.