Jump to main content

##

# 2.65.14 MCPWM_SecondaryEventCallbackRegister Function

## C

    void MCPWM_SecondaryEventCallbackRegister (MCPWM_CALLBACK callback, uintptr_t context)

## Summary

Registers the function to be called from secondary event interrupt

## Description

This function registers the callback function to be called from secondary event interrupt

## Precondition

MCPWM_Initialize() must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
callback | callback function pointer
context | Allows the caller to provide a context value (usually a pointer to the callers context for multi-instance clients)

## Returns

None.

## Example

    void MCPWM_Callback_Fn(uintptr_t context);

    MCPWM_Initialize();
    MCPWM_SecondaryEventCallbackRegister(MCPWM_Callback_Fn, NULL);

## Remarks

Context value can be set to NULL if not required. To disable callback function, pass NULL for the callback parameter.