Jump to main content

##

# 2.127.7 TSENS_ComparisonWindowSet Function

## C

    void TSENS_ComparisonWindowSet(uint32_t low_threshold, uint32_t high_threshold);

## Summary

Configures low threshold and high threshold window values

## Description

This function configures low and high threshold values of the window

## Precondition

TSENS_Initialize() function must have been called first for the associated instance

## Parameters

Param | Description
--- | ---
low_threshold | 24-bit value for lower threshold
high_threshold | 24-bit value for higher threshold

## Returns

None.

## Example

    TSENS_Initialize();
    TSENS_Enable();
    TSENS_ComparisionWindowSet(0, 3000);

## Remarks

Threshold values are in two's complement format and they are register values.