Jump to main content

##

# 2.72.11 NVM_ProgramFlashWriteProtectLock Function

## C

    void NVM_ProgramFlashWriteProtectLock( void )

## Summary

Disable Writes to Program Flash Write Protect Lock register

## Description

This Function will disable writes to write protect lock register. Once locked calling NVM_ProgramFlashWriteProtect() does not have any effect.

## Precondition

None

## Parameters

None

## Returns

None.

## Example

    NVM_ProgramFlashWriteProtectLock();

## Remarks

Writes to write protect lock register can be enabled only by Reset.