Jump to main content

##

# 2.113.2 SMC_DataAddressGet Function

## C

    uint32_t SMC_DataAddressGet(uint8_t chipSelect)

## Summary

Returns the External Bus Interface (EBI) address for the requested chip select number.

## Description

Returns the External Bus Interface (EBI) address for the requested chip select number.

## Precondition

None.

## Parameters

Param | Description
--- | ---
chipSelect | Chip select number

## Returns

Returns External Bus Interface (EBI) address

## Example

    SMC_DataAddressGet(3);

## Remarks

None.