Jump to main content

##

# 2.15.32 CLOCK_MonitorIsReady Function

## C

    inline static bool CLOCK_MonitorIsReady(CLOCK_MONITOR monitor);

## Summary

Checks if the clock monitor capture data is ready.

## Description

This inline function checks if the clock monitor capture data is ready.

## Precondition

None.

## Parameters

Param | Description
--- | ---
monitor | Instance of clock monitor

## Returns

true - clock capture data available

false - clock capture data not started or in progress

## Example

    bool readyStatus
    readyStatus = CLOCK_Monitor_IsReady(CLOCK_MONITOR_2);

## Remarks

None.