Jump to main content

##

# 2.51.13 GPIO_PinWrite Function

## C

    void GPIO_PinWrite(GPIO_PIN pin, bool value)

## Summary

Writes the logic level of the selected pin.

## Description

This function writes/drives the "value" on the selected I/O line/pin.

## Precondition

The desired pin must be configured as an output pin.

## Parameters

Param | Description
--- | ---
pin | One of the IO pins from the enum GPIO_PIN
value | value to be written on the selected pin:
- true | set pin to high (1).
- false | clear pin to low (0).

## Returns

None.

## Example

    GPIO_PinWrite(GPIO_PIN_RB3, true);

## Remarks

None.