Jump to main content

##

# 2.117.5 SUPC_ClearOutputPin Function

## C

    void SUPC_ClearOutputPin( SUPC_OUTPIN pin );

## Summary

Clears a specific output pin (OUTx) to logic LOW.

## Description

There are two pins controlled by the SUPC. This API helps to drive a logic LOW on a given OUTx pin.

## Precondition

None.

## Parameters

Param | Description
--- | ---
pin | Identifies the output pin to be cleared

## Returns

None.

## Example

    SUPC_ClearOutputPin( SUPC_OUTPIN_OUT0 );

## Remarks

None.