Jump to main content

##

# 2.91.14 QEIx_PhaseInputSwappedGet Function

## C

    /* x refers to the instance number */

    inline static bool QEIx_PhaseInputSwappedGet(void)

## Summary

Gets the status of QEI input phase swap configuration.

## Description

This function returns true if the QEA and QEB inputs were swapped before decoder logic and false otherwise.

## Precondition

QEI peripheral should be initialized and enabled properly.

## Parameters

None.

## Returns

true - Phase inputs are swapped.

false - Phase inputs are not swapped.

## Example

    QEI1_Initialize();
    QEI1_Enable();
    QEI1_PhaseInputSwappedGet();

## Remarks

None.