Jump to main content

##

# 2.4.8 ADCHS_ChannelConversionStart Function

## C

    void ADCHS_ChannelConversionStart(ADCHS_CHANNEL_NUM channel)

## Summary

Starts the ADC conversion of an analog channel

## Description

This function starts ADC conversion of an analog channel specified in channel.

## Precondition

ADCHS_Initialize() function must have been called first for the associated instance and ADC module corresponding to channel must have been enabled using ADCHS_ModulesEnable() function.

## Parameters

Param | Description
--- | ---
channel | analog channel

## Returns

None.

## Example

    ADCHS_Initialize();
    ADCHS_ModulelsEnable(ADCHS_MODULE0_MASK);
    ADCHS_ChannelConversionStart(ADCHS_CH0);

## Remarks

This function can be called at the start to generate initial trigger. This can also be used to trigger the conversion of an input without changing the trigger source.