Jump to main content

##

# 2.43.9 EVIC_ExternalInterruptDisable Function

## C

    void EVIC_ExternalInterruptDisable( EXTERNAL_INT_PIN extIntPin );

## Summary

Disables external interrupt on selected external interrupt pins.

## Description

This function disables external interrupt on selected external interrupt pins.

## Precondition

Iterrupt option for Corresponding pins must be enabled in EVIC manager.

## Parameters

Param | Description
--- | ---
extIntPin | One or multiple external interrupt pins ORed from the enum EXTERNAL_INT_PIN

## Returns

None.

## Example

    // Disable external interrupt for INT1 pin
    EVIC_ExternalInterruptDisable(EXTERNAL_INT_1);

## Remarks

None.