Jump to main content

##

# 2.47.55 FLEXCOMx_TWI_Initialize Function

## C

    /* x = FLEXCOM instance number */

    /* TWI master and slave mode */

    void FLEXCOMx_TWI_Initialize(void)

## Summary

Initializes the instance of the FLEXCOM TWI peripheral in either master or slave mode.

## Description

This function initializes the given instance of the FLEXCOM TWI peripheral as configured by the user from the MCC.

## Precondition

None

## Parameters

None.

## Returns

None.

## Example

    FLEXCOM0_TWI_Initialize();

## Remarks

Resets the FLEXCOM TWI module if it was already running and reinitializes it