Jump to main content

##

# 2.51.16 GPIO_PinToggle Function

## C

    void GPIO_PinToggle(GPIO_PIN pin)

## Summary

Toggles the selected pin.

## Description

This function toggles/inverts the value on the selected I/O line/pin.

## Precondition

Pin must be made output before toggling.

## Parameters

Param | Description
--- | ---
pin | One of the IO pins from the enum GPIO_PIN

## Returns

None.

## Example

    GPIO_PinToggle(GPIO_PIN_RB3);

## Remarks

None.