Jump to main content

##

# 2.83.11 PIT64B_DelayUs Function

## C

    /* x = PIT64B instance number */
    void PIT64Bx_DelayUs(uint32_t ms)

## Summary

Delays processing for x microseconds.

## Description

Delays execution by using the PIT64B timer to determine when given number of microseconds has expired.

## Precondition

PIT64B is configured and enabled. The PIT64B interrupt is also enabled.

## Parameters

Param | Description
--- | ---
us | number of microseconds to delay

## Returns

None.