Jump to main content

##

# 2.89.9 PWMx_ClkSelect Function

## C

    /* x = PWM instance number */

    void PWMx_ClkSelect (PWM_CLK_SEL pwmClk)

## Summary

Selects the clock source for the PWM peripheral

## Description

Selects the clock source for the PWM peripheral. The source clock can be selected between 100 KHz slow clock and 48 MHz fast clock.

## Precondition

None

## Parameters

Param | Description
--- | ---
pwmClk | PWM clock source of type PWM_CLK_SEL

## Returns

None

## Example

    PWM0_ClkSelect(PWM_CLK_SEL_LOW_100KHZ);

## Remarks

None