Jump to main content

##

# 2.3.72 ADCx_CompareStatusGet Function

## C

    // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.
    inline static bool ADCx_CompareStatusGet(ADCx_CHANNEL channel);

## Summary

Returns the status of the comparator.

## Description

This function returns the status of the comparator.

## Precondition

None.

## Parameters

Param | Description
--- | ---
channel | Selected channel

## Returns

true - If Compare status is true

false - If Compare status is false

## Example

    bool cmpStatus;
    cmpStatus = ADC1_CompareStatusGet(ADC1_CHANNEL0);

## Remarks

None