Jump to main content

##

# 2.3.29 ADC_CompareWinThresholdSet Function

## C

    void ADC_CompareWinThresholdSet(ADC_CORE_NUM core, uint16_t low_threshold, uint16_t high_threshold)

## Summary

Configures the low and high threshold values for the comparator on the specified ADC core

## Description

This function lets the application configure the low and high threshold values for the comparator on the specified ADC core

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
core | ADC core n
low_threshold | lower threshold of the ADC core n digital comparator
high_threshold | higher threshold of the ADC core n digital comparator

## Returns

None.

## Example

    ADC_CompareWinThresholdSet(ADC_CORE_NUM1, 0x100, 0x200);

## Remarks

None