Jump to main content

##

# 2.64.17 MCANx_InterruptClear Function

## C

    void MCANx_InterruptClear(MCAN_INTERRUPT_MASK interruptMask) // x - Instance of the MCAN peripheral

## Summary

Clears Interrupt status.

## Precondition

MCANx_Initialize must have been called for the associated MCAN instance.

## Parameters

Param | Description
--- | ---
interruptMask | Interrupt to be cleared

## Returns

None

## Example

    MCAN_INTERRUPT_MASK interruptMask = MCAN_INTERRUPT_RF0W_MASK;
    MCAN0_InterruptClear(interruptMask);

## Remarks

None.