Jump to main content

##

# 2.78.2 PAC_PeripheralIsProtected Function

## C

    bool PAC_PeripheralIsProtected( PAC_PERIPHERAL peripheral );

## Summary

Returns PAC protection status of peripheral.

## Description

This function returns status PAC protection status for the specified peripheral.

## Precondition

On some devices PAC_Initialize() function needs to be called first.

## Parameters

Param | Description
--- | ---
peripheral | Peripheral to be operated on.

## Returns

true - Peripheral is protected.

false - Peripheral is not protected.

## Example

    bool status = false;

    status = PAC_PeripheralIsProtected(PAC_PERIPHERAL_DSU);

## Remarks

None.