Jump to main content

##

# 2.86.8 PORT_PinInputEnable Function

## C

    void PORT_PinInputEnable(PORT_PIN pin)

## Summary

Configures the selected IO pin as input.

## Description

This function configures the selected IO pin as input. This function override the MCC input output pin settings.

## Precondition

The PORT_Initialize() function should have been called.

## Parameters

Param | Description
--- | ---
pin | One of the IO pins from the enum PORT_PIN.

## Returns

None.

## Example

    PORT_PinInputEnable(PORT_PIN_PB03);

## Remarks

None.