Jump to main content

##

# 2.117.11 SUPC_GPBRRead Function

## C

    uint32_t SUPC_GPBRRead (GPBR_REGS_INDEX reg);

## Summary

Reads the data from General Purpose Backup Register(GPBR)

## Description

This functions is used to read the data available in GPBR register when the device wakeup from Low power modes.

## Precondition

None

## Parameters

Param | Description
--- | ---
reg | Identifies the GPBR register

## Returns

32 bit data available in specified GPBR register.

## Example

    uint32_t data;

    data = SUPC_GPBRRead (GPBR_REGS_2);

## Remarks

None.