Jump to main content

##

# 2.8.79 CANx_StandardFilterElementSet Function

## C

    bool CANx_StandardFilterElementSet(uint8_t filterNumber, can_sidfe_registers_t *stdMsgIDFilterElement) // x - Instance of the CAN peripheral

## Summary

Set a standard filter element configuration.

## Precondition

CANx_Initialize and CANx_MessageRAMConfigSet must have been called for the associated CAN instance.

## Parameters

Param | Description
--- | ---
filterNumber | Standard Filter number to be configured
stdMsgIDFilterElement | Pointer to Standard Filter Element configuration to be set on specific filterNumber

## Returns

Request status. true - Request was successful

false - Request has failed

## Example

    can_sidfe_registers_t stdMsgIDFilterElement;
    stdMsgIDFilterElement.CAN_SIDFE_0 = 0x00;
    CAN0_StandardFilterElementSet(1, &stdMsgIDFilterElement);

## Remarks

None.