Jump to main content

##

# 2.72.6 NVM_DoubleWordWrite Function

## C

    bool NVM_DoubleWordWrite( uint32_t *data, const uint32_t address );

## Summary

Writes two words into the Flash.

## Description

Writes two words (8 bytes) at the given address.

## Precondition

None

## Parameters

Param | Description
--- | ---
data | Pointer to the buffer which holds data to be written.
address | Address at which the data will be written.

## Returns

Always return true.

## Example

    NVM_DoubleWordWrite(data_to_fill, 0x9D100000);