Jump to main content

##

# 2.99.56 RTC_RTCCTimeStampGet Function

## C

    void RTC_RTCCTimeStampGet( struct tm * timeStamp );

## Summary

Get the Time stamp of Tamper Detection.

## Description

This function is used to get the recorded Time Stamp of the tamper Detection.

## Precondition

Tamper channels must be configured properly using MCC.

## Parameters

Param | Description
--- | ---
timeStamp | Time structure to be filled

## Returns

None.

## Example

    struct tm currentTime;
    RTC_RTCCTimeStampGet(&currentTime);

## Remarks

This Feature may not be available on all devices. Refer to device Datasheet for more information.