Jump to main content

##

# 2.3.44 ADC_FIFORead Function

## C

    uint32_t ADC_FIFORead(void)

## Summary

Returns a single ADC conversion value from the ADC FIFO

## Description

Returns a single ADC conversion value from the ADC FIFO

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

None

## Returns

uint32_t - ADC result value

## Example

    uint32_t adc_result;

    if (ADC_EOSStatusGet(ADC_CORE_NUM1))
    {
        // ADC conversion is complete. Read the conversion result.

        adc_result = ADC_FIFORead();
    }

## Remarks

None