Jump to main content

##

# 2.11.31 CCPx_Compare16bitPeriodValueGet Function

## C

    /* x = CCP instance number */

    uint16_t CCPx_Compare16bitPeriodValueGet( void )

## Summary

Reads the period value of given timer.

## Description

This function reads the value of period.

## Precondition

CCPx_CompareInitialize() function must have been called first.

## Parameters

None.

## Returns

uint16_t - The timer's period value.

## Example

    uint16_t period = 0;
    CCP1_CompareInitialize();
    period = CCP1_Compare16bitPeriodValueGet();

## Remarks

The caller must know the number of significant bytes of timer. Period value is right-aligned.