Jump to main content

##

# 2.8.51 CANx_InterruptClear Function

## C

    void CANx_InterruptClear(CAN_INTERRUPT_MASK interruptMask) // x - Instance of the CAN peripheral

## Summary

Clears Interrupt status.

## Precondition

CANx_Initialize must have been called for the associated CAN instance.

## Parameters

Param | Description
--- | ---
interruptMask | Interrupt to be cleared

## Returns

None

## Example

    CAN_INTERRUPT_MASK interruptMask = CAN_INTERRUPT_RF0W_MASK;
    CAN0_InterruptClear(interruptMask);

## Remarks

None.