Jump to main content

##

# 2.61.25 LCDCx_SetClockDivider Function

## C

    // x - Instance of the LCDC peripheral

    void LCDCx_SetClockDivider(uint8_t value)

## Summary

Sets the clock divider for the pixel clock

## Description

The pixel clock period formula is LCDPCLK = source clock / value when source clock is the system clock when CLKSET is '0', and 2x system_clock when CLKSEL is '1'

## Precondition

None.

## Parameters

Param | Description
--- | ---
value | the 8-bit divider value, must be greater than 2

## Returns

None

## Remarks

None