Jump to main content

##

# 2.121.64 TCCx_PWM24bitCounterSet Function

## C

    /* x = TCC instance number */
    void TCCx_PWM24bitCounterSet(uint32_t count);

## Summary

Sets the counter value of a given TCC instance

## Description

This function updates the counter value.

## Precondition

TCCx_PWMInitialize function must have been called first for the given channel.

## Parameters

Param | Description
--- | ---
count | counter value

## Returns

None

## Example

    TCC0_PWMInitialize();
    TCC0_PWM24bitCounterSet(0x100U);

## Remarks

This function waits till sync operation is complete.