Jump to main content

##

# 2.55.2 HTMx_PeriodGet Function

## C

    /* x = HTM timer instance number */
    uint16_t HTMx_PeriodGet(void)

## Summary

Returns the period value for the HTM timer

## Description

Returns the value of the pre-load register

## Precondition

HTMx_Initialize() function must have been called first.

## Parameters

None

## Returns

16-bit timer period value

## Example

    uint16_t period = HTM0_PeriodGet();

## Remarks

None