Jump to main content

##

# 2.11.37 CCPx_Capture32bitBufferRead Function

## C

    /* x = CCP instance number */

    uint32_t CCPx_Capture32bitBufferRead( void );

## Summary

Reads 32 bit capture value.

## Description

This function reads the 32 bit captured value. Value can be read from interrupt routine or by polling.

## Precondition

CCPx_CaptureInitialize() function must have been called first.

## Parameters

None.

## Returns

uint32_t - 32 bit Captured value.

## Example

    uint32_t captureValue = 0;
    CCP1_CaptureInitialize();
    CCP1_CaptureStart();
    captureValue = CCP1_Capture32bitBufferRead();

## Remarks

None.