Jump to main content

##

# 2.53.3 HEMC_DisableECC Function

## C

    bool HEMC_DisableECC( uint8_t chipSelect )

## Summary

Disable the ECC for the given chip select.

## Description

This function disable the ECC for the given chip select of the HEMC peripheral.

## Precondition

None.

## Parameters

Param | Description
--- | ---
chipSelect | The chip select for which ECC is disabled.

## Returns

True if ECC was disable for this chip select, False otherwise.

## Example

    HEMC_DisableECC(0);

## Remarks

None.