Jump to main content

##

# 2.83.10 PIT64B_DelayMs Function

## C

    /* x = PIT64B instance number */
    void PIT64Bx_DelayMs(uint32_t ms)

## Summary

Delays processing for x milliseconds.

## Description

Delays execution by using the PIT64B timer to determine when given number of milliseconds has expired.

## Precondition

PIT64B is configured and enabled. The PIT64B interrupt is also enabled.

## Parameters

Param | Description
--- | ---
ms | number of milliseconds to delay

## Returns

None.