Jump to main content

##

# 2.52.6 HEFC_IsBusy Function

## C

    bool HEFC_IsBusy(void)

## Summary

Returns the current status of HEFC controller.

## Description

This function is used to check is HEFC is busy or not

## Precondition

None.

## Parameters

None

## Returns

true: If HEFC peripheral is busy doing an operation.

false: If HEFC peripheral is ready to accept new request..

## Example

    HEFC_SectorErase( 0x10010000 );

    while(HEFC_IsBusy());