Jump to main content

##

# 2.72.9 NVM_ProgramFlashSwapBank Function

## C

    void NVM_ProgramFlashSwapBank( void )

## Summary

Swaps the Program Flash Bank 2

## Description

This function will map the Program flash bank 2 to lower region. This function should be placed in boot flash memroy and needs to be called from boot flash memory after reset before jumping to program flash memory.

## Precondition

None

## Parameters

None

## Returns

None.

## Example

    NVM_ProgramFlashSwapBank();