Jump to main content

##

# 2.39.17 GIRQ_AGG_INT_NUM_GET macro

## C

    #define GIRQ_AGG_INT_NUM_GET(int_src)       ((((uint32_t)(int_src)) & ((uint32_t)0xFF << 8U)) >> 8U)

## Summary

This macro returns the aggregate NVIC interrupt number from the given interrupt source.

## Description

This macro returns the aggregate NVIC interrupt number from the given interrupt source which must be of type ECIA_INT_SOURCE

## Remarks

None