Jump to main content

##

# 2.3.102 ADC_WINMODE Enum

## C

    typedef enum
    {
        /* Window comparison is disabled */
        ADC_WINMODE_DISABLED = ADC_CTRLB_WINMODE_DISABLE_Val,
        /* Result is greater than lower threshold */
        ADC_WINMODE_GREATER_THAN_WINLT = ADC_CTRLB_WINMODE_MODE1_Val,
        /* Result is less than upper threshold */
        ADC_WINMODE_LESS_THAN_WINUT = ADC_CTRLB_WINMODE_MODE2_Val,
        /* Result is in between lower threshold and upper threshold */
        ADC_WINMODE_BETWEEN_WINLT_AND_WINUT = ADC_CTRLB_WINMODE_MODE3_Val,
        /* Result is outside lower threshold and upper threshold */
        ADC_WINMODE_OUTSIDE_WINLT_AND_WINUT = ADC_CTRLB_WINMODE_MODE4_Val
    }ADC_WINMODE;

## Summary

Identifies ADC window comparison modes

## Description

Enum for the ADC window comparison mode. This can be used in the API to change the window mode runtime.

## Remarks

None.