Jump to main content

##

# 2.75.13 OPA_OUTPUT_VOLTAGE_OFFSET_CORRECTION Enum

## C

    typedef enum
    {
    DECREASE_15_UNIT_VOLTAGE = 0xf,
    DECREASE_14_UNIT_VOLTAGE = 0xe,
    DECREASE_13_UNIT_VOLTAGE = 0xd,
    DECREASE_12_UNIT_VOLTAGE = 0xc,
    DECREASE_11_UNIT_VOLTAGE = 0xb,
    DECREASE_10_UNIT_VOLTAGE = 0xa,
    DECREASE_9_UNIT_VOLTAGE = 0x9,
    DECREASE_8_UNIT_VOLTAGE = 0x8,
    DECREASE_7_UNIT_VOLTAGE = 0x7,
    DECREASE_6_UNIT_VOLTAGE = 0x6,
    DECREASE_5_UNIT_VOLTAGE = 0x5,
    DECREASE_4_UNIT_VOLTAGE = 0x4,
    DECREASE_3_UNIT_VOLTAGE = 0x3,
    DECREASE_2_UNIT_VOLTAGE = 0x2,
    DECREASE_1_UNIT_VOLTAGE = 0x1,
    NO_CORRECTION = 0x0,
    INCREASE_1_UNIT_VOLTAGE = 0x1e,
    INCREASE_2_UNIT_VOLTAGE = 0x1d,
    INCREASE_3_UNIT_VOLTAGE = 0x1c,
    INCREASE_4_UNIT_VOLTAGE = 0x1b,
    INCREASE_5_UNIT_VOLTAGE = 0x1a,
    INCREASE_6_UNIT_VOLTAGE = 0x19,
    INCREASE_7_UNIT_VOLTAGE = 0x18,
    INCREASE_8_UNIT_VOLTAGE = 0x17,
    INCREASE_9_UNIT_VOLTAGE = 0x16,
    INCREASE_10_UNIT_VOLTAGE = 0x15,
    INCREASE_11_UNIT_VOLTAGE = 0x14,
    INCREASE_12_UNIT_VOLTAGE = 0x13,
    INCREASE_13_UNIT_VOLTAGE = 0x12,
    INCREASE_14_UNIT_VOLTAGE = 0x11,
    INCREASE_15_UNIT_VOLTAGE = 0x10,

    } OPA_OUTPUT_VOLTAGE_OFFSET_CORRECTION;

## Summary

Enumeration for selecting the output voltage offset correction for the OPA module.

## Description

This enumeration defines the possible output voltage offset correction settings for the OPA module.

## Remarks

None.