Jump to main content

##

# 2.121.52 TCCx_Capture32bitValueGet Function

## C

    /* x = TCC instance number */
    uint32_t TCCx_Capture32bitValueGet( TCCx_CHANNEL_NUM channel );

## Summary

Reads capture value from given channel

## Description

This function reads the captured value stored in CC[x]. Value can be read from interrupt routine or by polling.

## Precondition

TCCx_CaptureInitialize() function must have been called first.

## Parameters

Param | Description
--- | ---
channel | capture channel number

## Returns

Captured value from given channel

## Example

    uint32_t captureValue = 0;
    TCC0_CaptureInitialize();
    TCC0_CaptureStart();
    captureValue = TCC0_Capture32bitValueGet(TCC0_CHANNEL0);

## Remarks

None.