Jump to main content

##

# 2.39.4 ECIA_GIRQBlockEnable Function

## C

    void ECIA_GIRQBlockEnable(ECIA_GIRQ_BLOCK_NUM block)

## Summary

Enables the given GIRQ block

## Description

Enables the interruput generation from the given GIRQ block to NVIC

## Precondition

None.

## Parameters

Param | Description
--- | ---
block | One of the GIRQ block number from the enum ECIA_GIRQ_BLOCK_NUM

## Returns

None

## Example

    ECIA_GIRQBlockEnable(ECIA_GIRQ_BLOCK_NUM8);

## Remarks

None