Jump to main content

##

# 2.72.4 NVM_WordWrite Function

## C

    bool NVM_WordWrite( uint32_t data, const uint32_t address );

## Summary

Writes One word into the Flash.

## Description

Writes one word (4 bytes) at the given address.

## Precondition

None

## Parameters

Param | Description
--- | ---
data | Data to be written.
address | Address at which the data will be written.

## Returns

Always return true.

## Example

    NVM_WordWrite(data_to_fill, 0x9D100000);