Jump to main content

##

# 2.53.19 HEMC_Read16 Function

## C

    void HEMC_Read16(uint32_t dataAddress)

## Summary

Read 16 bit data at the given address.

## Description

Read 16 bit data at the given address.

## Precondition

None.

## Parameters

Param | Description
--- | ---
dataAddress | Address were data is read.

## Returns

Read data.

## Example

    uint16_t data = HEMC_Read16((uint32_t)(0x60000000U));

## Remarks

None.