Jump to main content

##

# 2.8.48 CANx_ExtendedFilterElementGet Function

## C

    bool CANx_ExtendedFilterElementGet(uint8_t filterNumber, can_xidfe_registers_t *extMsgIDFilterElement) // x - Instance of the CAN peripheral

## Summary

Get a Extended filter element configuration.

## Precondition

CANx_Initialize and CANx_MessageRAMConfigSet must have been called for the associated CAN instance.

## Parameters

Param | Description
--- | ---
filterNumber | Extended Filter number to get filter configuration.
extMsgIDFilterElement | Pointer to Extended Filter Element configuration for storing filter configuration.

## Returns

Request status. true - Request was successful

false - Request has failed

## Example

    can_xidfe_registers_t extMsgIDFilterElement;
    CAN0_ExtendedFilterElementGet(1, &extMsgIDFilterElement);

## Remarks

None.