Jump to main content

##

# 2.4.9 ADCHS_GlobalEdgeConversionStart Function

## C

    void ADCHS_GlobalEdgeConversionStart(void)

## Summary

Starts the ADC conversion of analog channels configured for global software edge trigger

## Description

This function sets the global edge software trigger bit. This starts ADC conversion of analog channels configured for global software edge trigger.

## Precondition

ADCHS_Initialize() function must have been called first for the associated instance and ADC modules corresponding to channels must have been enabled using ADCHS_ModulesEnable() function.

## Parameters

None.

## Returns

None.

## Example

    ADCHS_Initialize();
    ADCHS_ModulelsEnable(ADCHS_MODULE0_MASK);
    ADCHS_GlobalEdgeConversionStart();

## Remarks

None