Jump to main content

##

# 2.3.47 ADC_GlobalInterruptsStatusGet Function

## C

    ADC_GLOBAL_INT ADC_GlobalInterruptsStatusGet(void)

## Summary

Returns the global interrupt status

## Description

This function returns the global interrupt status

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

None

## Returns

ADC_GLOBAL_INT - bitwise OR of the following macros indicating global interrupt event status: ADC_GLOBAL_INT_PFFHFUL ADC_GLOBAL_INT_PFFRDY ADC_GLOBAL_INT_PFFOVF ADC_GLOBAL_INT_PFFUNF ADC_GLOBAL_INT_VREFRDY ADC_GLOBAL_INT_VREFUPD ADC_GLOBAL_INT_CRRDY1

## Example

    ADC_GLOBAL_INT adcGlobalIntStatus;

    adcGlobalIntStatus = ADC_GlobalInterruptsStatusGet();

## Remarks

None