Jump to main content

##

# 2.49.6 GENERIC_TIMER_PeriodSet Function

## C

    void GENERIC_TIMER_PeriodSet(uint64_t period);

## Summary

Set the timer period value.

## Description

This function sets the timer period value.

## Precondition

None.

## Parameters

Param | Description
--- | ---
period | The period value of generic timer. For example, if the timer is running at a frequency of 24 MHz and if the desired timeout is 10 milliseconds, then the period value must be specified as 24MHz x (10/1000) = 240000 cycles

## Returns

None.